EESchema-DOCLIB  Version 2.0
#
$CMP STM6822x
D 5-pin supervisor with watchdog timer and push-button reset
K supervisor, watchdog, reset
F https://www.st.com/content/ccc/resource/technical/document/datasheet/group0/7f/60/27/e3/bf/f2/4e/2c/CD00047783/files/CD00047783.pdf/jcr:content/translations/en.CD00047783.pdf
$ENDCMP
#
#End Doc Library
