(module ITDB02-3.2WD (layer F.Cu) (tedit 56C6AB88)
  (fp_text reference U6 (at -0.7 -6.575) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ITDB02-3.2WD (at 9.3 -6.575) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 240px (at 77.1 23.225) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 400px (at 43.4 2.825) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3.2" (at 44 22.525) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.1 47.125) (end 80.1 1.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.1 47.125) (end 9.1 1.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 80.1 47.225) (end 9.1 47.125) (layer F.SilkS) (width 0.15))
  (fp_line (start 80.1 1.225) (end 80.1 47.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.1 1.225) (end 80.1 1.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.9 54.025) (end -2.9 -5.775) (layer F.SilkS) (width 0.15))
  (fp_line (start 92.1 54.025) (end -2.9 54.025) (layer F.SilkS) (width 0.15))
  (fp_line (start 92.1 -5.775) (end 92.1 54.025) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.9 -5.775) (end 92.1 -5.775) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.75 -1.7504) (end -1.75 50.0496) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3 -1.7504) (end 4.3 50.0496) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.7504) (end 4.3 -1.7504) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 50.0496) (end 4.3 50.0496) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.81 49.5296) (end 3.81 -1.2704) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 1.2696) (end -1.27 49.5296) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.81 49.5296) (end -1.27 49.5296) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.81 -1.2704) (end 1.27 -1.2704) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -1.5504) (end -1.55 -1.5504) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -1.2704) (end 1.27 1.2696) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 1.2696) (end -1.27 1.2696) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.55 -1.5504) (end -1.55 -0.0004) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 -0.0004) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 2.54 -0.0004) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at 0 2.5396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole oval (at 2.54 2.5396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole oval (at 0 5.0796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole oval (at 2.54 5.0796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole oval (at 0 7.6196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole oval (at 2.54 7.6196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole oval (at 0 10.1596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole oval (at 2.54 10.1596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole oval (at 0 12.6996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole oval (at 2.54 12.6996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole oval (at 0 15.2396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole oval (at 2.54 15.2396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole oval (at 0 17.7796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole oval (at 2.54 17.7796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole oval (at 0 20.3196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 18 thru_hole oval (at 2.54 20.3196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 19 thru_hole oval (at 0 22.8596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 20 thru_hole oval (at 2.54 22.8596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 21 thru_hole oval (at 0 25.3996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 22 thru_hole oval (at 2.54 25.3996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 23 thru_hole oval (at 0 27.9396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 24 thru_hole oval (at 2.54 27.9396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 25 thru_hole oval (at 0 30.4796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 26 thru_hole oval (at 2.54 30.4796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 27 thru_hole oval (at 0 33.0196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 28 thru_hole oval (at 2.54 33.0196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 29 thru_hole oval (at 0 35.5596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 30 thru_hole oval (at 2.54 35.5596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 31 thru_hole oval (at 0 38.0996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 32 thru_hole oval (at 2.54 38.0996) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 33 thru_hole oval (at 0 40.6396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 34 thru_hole oval (at 2.54 40.6396) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 35 thru_hole oval (at 0 43.1796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 36 thru_hole oval (at 2.54 43.1796) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 37 thru_hole oval (at 0 45.7196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 38 thru_hole oval (at 2.54 45.7196) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 39 thru_hole oval (at 0 48.2596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 40 thru_hole oval (at 2.54 48.2596) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 9.1 -2.775) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 9.1 51.025) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 80.1 -2.775) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 80.1 51.025) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
    (at (xyz 0.05 -0.95 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
