(module FerroCore_DJNR4018_Series (layer F.Cu) (tedit 5DC69974)
  (fp_text reference REF** (at 0 -3.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FerroCore_DJNR4018_Series (at 0 -4.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.3 -2.3) (end 2.3 -2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.3 -2.3) (end 2.3 2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.3 2.3) (end -2.3 2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.3 -2.3) (end -2.3 2.3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask))
)
