(module 2450AT18D0100E_2.45GHz_Antenna (layer F.Cu) (tedit 619A65E7)
  (zone_connect 2)
  (fp_text reference REF** (at 0 -4.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 2450AT18D0100E_2.45GHz_Antenna (at 0 -2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.75 0.25) (end 3.75 -0.25) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.75 -1.5) (end 3.75 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 -1) (end -0.75 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 0.5) (end -0.25 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 0) (end -0.75 0.5) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at 0 0) (size 1 0.6) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 2 smd rect (at 3 0) (size 1 0.6) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 2 smd rect (at 3 -1.3) (size 1 0.6) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 2 smd rect (at 0 -1.3) (size 1 0.6) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 2 smd rect (at 4 1.4) (size 1 6) (layers F.Cu)
    (zone_connect 2))
  (pad 2 smd rect (at 1.5 4.9) (size 6 1) (layers F.Cu)
    (zone_connect 2))
  (pad 2 smd rect (at -1 2.65) (size 1 3.5) (layers F.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 4 -0.7) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 4 0.7) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 4 2.1) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 4 3.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 4 4.9) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 2.5 4.9) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 1.2 4.9) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 0 4.9) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at -1 3.7) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at -1 1.3) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at -1 2.3) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
  (pad 2 thru_hole circle (at -1 4.9) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2))
)
