(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "AD8314" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD8314" (id 1) (at 12.7 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8314.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Detector/Controller" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD8314_0_0"
      (rectangle (start 0 0) (end 25.4 -15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "AD8314_1_1"
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "RFIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -6.35 0) (length 5.08)
        (name "ENBL" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -8.89 0) (length 5.08)
        (name "VSET" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -2.54 180) (length 5.08)
        (name "FILTR" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 30.48 -12.7 180) (length 5.08)
        (name "COMM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 30.48 -5.08 180) (length 5.08)
        (name "V_UP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 30.48 -7.62 180) (length 5.08)
        (name "V_DN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "VPOS" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BGA420" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "BGA420" (id 1) (at 11.43 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -1.27 1.27 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at -1.27 1.27 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_fp_filters" "shimatta_smd:BGA420-INF" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BGA420_0_1"
      (rectangle (start 0 0) (end 13.97 -12.7)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "BGA420_1_1"
      (pin input line (at -5.08 -6.35 0) (length 5.08)
        (name "RFIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -17.78 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 19.05 -6.35 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 5.08 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HMC154S8" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "HMC154S8" (id 1) (at 10.16 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.qsl.net/n9zia/trans/hmc154s8.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "rf,switch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LOW DISTORTION T/R SWITCH DC - 2.5 GHZ" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HMC154S8_0_0"
      (polyline
        (pts
          (xy 11.43 -11.43)
          (xy 15.24 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -8.89)
          (xy 15.24 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 15.24 -11.43)
          (xy 17.78 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 15.24 -8.89)
          (xy 17.78 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy 6.35 -5.08)
          (xy 7.62 -5.08)
          (xy 7.62 -7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy 7.62 -2.54)
          (xy 8.89 -2.54)
          (xy 8.89 -7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "SW" (at 8.89 -10.16 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "HMC154S8_0_1"
      (polyline
        (pts
          (xy 0 -10.16)
          (xy 6.35 -10.16)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 17.78 -22.86)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 6.35 -7.62) (end 11.43 -12.7)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "HMC154S8_1_1"
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "RF" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 22.86 -2.54 180) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -8.89 180) (length 5.08)
        (name "RF1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 -27.94 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 -27.94 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -11.43 180) (length 5.08)
        (name "RF2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX2644" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX2644" (id 1) (at 15.24 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2644.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "lna,rf,amplifier,amp,maxim" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.45 GHz LNA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX2644_0_0"
      (polyline
        (pts
          (xy 8.128 -3.556)
          (xy 0.762 -3.556)
          (xy 0.762 -2.54)
          (xy 0 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "50 Ohm" (at 16.51 -11.684 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "bias" (at 10.414 -3.556 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "MAX2644_0_1"
      (polyline
        (pts
          (xy 0 -10.16)
          (xy 7.874 -10.16)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -8.636)
          (xy 10.16 -4.572)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 20.32 -10.16)
          (xy 12.446 -10.16)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.874 -10.16)
          (xy 7.874 -7.112)
          (xy 12.446 -10.16)
          (xy 7.874 -13.208)
          (xy 7.874 -10.16)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 10.16 -4.572)
          (xy 8.128 -4.572)
          (xy 8.128 -2.54)
          (xy 12.954 -2.54)
          (xy 12.954 -4.572)
          (xy 10.16 -4.572)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 20.32 -22.86)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX2644_1_1"
      (pin unspecified line (at -5.08 -2.54 0) (length 5.08)
        (name "BIAS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -17.78 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -10.16 0) (length 5.08)
        (name "RFIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -20.32 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -10.16 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX2750" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX2750" (id 1) (at 7.62 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX2750_0_1"
      (rectangle (start 0 0) (end 17.78 -11.43)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MAX2750_1_1"
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "BYP" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "TUNE" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -10.16 0) (length 5.08)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -10.16 180) (length 5.08)
        (name "VCC1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -7.62 180) (length 5.08)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -5.08 180) (length 5.08)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -2.54 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NRF24L01" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -11.43 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "NRF24L01" (id 1) (at 5.08 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm" (id 2) (at 5.08 20.32 0)
      (effects (font (size 1.27 1.27) italic) (justify left) hide)
    )
    (property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2730/34105/file/nRF24L01_Product_Specification_v2_0.pdf" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low Power RF Transciever" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ultra low power 2.4GHz RF Transceiver, QFN20 4x4mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*4x4*0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NRF24L01_0_1"
      (rectangle (start -11.43 16.51) (end 11.43 -16.51)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 4.445)
          (xy 0 1.27)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 0 5.08) (radius 0.635)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (arc (start 1.27 5.08) (mid 0.9071 5.9946) (end 0 6.35)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 1.905 4.445) (mid 1.4313 6.5254) (end -0.635 6.985)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 2.54 3.81) (mid 2.008 7.088) (end -1.27 7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 11.43 -13.97) (end 11.43 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "NRF24L01_1_1"
      (pin input line (at -15.24 0 0) (length 3.81)
        (name "CE" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -7.62 180) (length 3.81)
        (name "XC1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 15.24 12.7 180) (length 3.81)
        (name "VDD_PA" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 7.62 180) (length 3.81)
        (name "ANT1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 2.54 180) (length 3.81)
        (name "ANT2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 3.81)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 -7.62 0) (length 3.81)
        (name "IREF" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -20.32 90) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 20.32 270) (length 3.81)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -15.24 -12.7 0) (length 3.81)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 3.81)
        (name "CSN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -20.32 90) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -2.54 180) (length 5.08)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -15.24 7.62 0) (length 3.81)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 12.7 0) (length 3.81)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -15.24 10.16 0) (length 3.81)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -15.24 -2.54 0) (length 3.81)
        (name "IRQ" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 20.32 270) (length 3.81)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -20.32 90) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -12.7 180) (length 3.81)
        (name "XC2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "nRF24L01P" (extends "NRF24L01")
    (property "Reference" "U" (id 0) (at -11.43 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "nRF24L01P" (id 1) (at 5.08 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm" (id 2) (at 5.08 20.32 0)
      (effects (font (size 1.27 1.27) italic) (justify left) hide)
    )
    (property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2726/34069/file/nRF24L01P_Product_Specification_1_0.pdf" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low Power RF Transciever" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "nRF24L01+, Ultra low power 2.4GHz RF Transceiver, QFN20 4x4mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*4x4*0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "NSVF4020SG4" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (id 0) (at -1.27 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NSVF4020SG4" (id 1) (at 8.89 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NSVF4020SG4_0_1"
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 3.81 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "NSVF4020SG4_1_1"
      (polyline
        (pts
          (xy -0.635 0.635)
          (xy 1.27 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -0.635)
          (xy 1.27 -2.54)
          (xy 1.27 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 1.905)
          (xy -0.635 -1.905)
          (xy -0.635 -1.905)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -1.778)
          (xy 0.508 -1.27)
          (xy 1.016 -2.286)
          (xy 0 -1.778)
          (xy 0 -1.778)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 0 0) (radius 2.8194)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin passive line (at 1.27 5.08 270) (length 2.54)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 1.27 -5.08 90) (length 2.54)
        (name "E" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.35 0 0) (length 5.715)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.81 -5.08 90) (length 2.54)
        (name "E" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RF2126" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RF2126" (id 1) (at 6.35 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RF2126_0_1"
      (rectangle (start 0 0) (end 22.86 -11.43)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "RF2126_1_1"
      (pin input line (at -5.08 -1.27 0) (length 5.08)
        (name "RFIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -3.81 0) (length 5.08)
        (name "RFIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -7.62 0) (length 5.08)
        (name "PC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -10.16 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -6.35 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -3.81 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -1.27 180) (length 5.08)
        (name "RFOUT" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -16.51 90) (length 5.08)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SE2436" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 13.97 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SE2436" (id 1) (at 13.97 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SE2436_0_1"
      (rectangle (start 0 0) (end 26.67 -55.88)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SE2436_1_1"
      (pin input line (at -5.08 -34.29 0) (length 5.08)
        (name "ANT_SEL" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -31.75 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -26.67 0) (length 5.08)
        (name "CPS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -22.86 180) (length 5.08)
        (name "VCC3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 31.75 -46.99 180) (length 5.08)
        (name "DNC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 31.75 -49.53 180) (length 5.08)
        (name "DNC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 31.75 -52.07 180) (length 5.08)
        (name "DNC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 31.75 -54.61 180) (length 5.08)
        (name "DNC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -34.29 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 31.75 -8.89 180) (length 5.08)
        (name "AUX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -6.35 180) (length 5.08)
        (name "ANT2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -36.83 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -3.81 180) (length 5.08)
        (name "ANT1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -39.37 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 31.75 -44.45 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 31.75 -41.91 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -60.96 90) (length 5.08)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "TRP" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -7.62 0) (length 5.08)
        (name "TRN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -31.75 0) (length 5.08)
        (name "CRX" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -17.78 180) (length 5.08)
        (name "VCC1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -24.13 0) (length 5.08)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -20.32 180) (length 5.08)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -29.21 0) (length 5.08)
        (name "CTX" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Wilkinson-2.4GHz" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 15.24 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Wilkinson-2.4GHz" (id 1) (at 5.08 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Wilkinson-2.4GHz_0_1"
      (polyline
        (pts
          (xy 0 -6.35)
          (xy 11.43 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -6.35)
          (xy 11.43 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 9.525 -8.89)
          (xy 9.525 -10.541)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 9.525 -5.08)
          (xy 9.525 -3.175)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.89 -5.08)
          (xy 10.16 -5.08)
          (xy 10.16 -7.62)
          (xy 10.16 -8.89)
          (xy 8.89 -8.89)
          (xy 8.89 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 11.43 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Wilkinson-2.4GHz_1_1"
      (pin input line (at -5.08 -6.35 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -2.54 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -11.43 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
