(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "OSC" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 -2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "OSC" (id 1) (at 15.24 -2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 5.08 -3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at 5.08 -3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "OSC_1_1"
      (polyline
        (pts
          (xy 4.826 9.398)
          (xy 6.604 9.398)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.715 6.35)
          (xy 5.715 8.382)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.715 11.43)
          (xy 5.715 9.398)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.604 8.382)
          (xy 4.826 8.382)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 6.35)
          (xy 5.715 6.35)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 11.43)
          (xy 5.715 11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 14.605 8.89)
          (xy 13.97 8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 14.478 13.97)
          (xy 11.176 13.97)
          (xy 11.176 10.668)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 12.7)
          (xy 7.62 5.08)
          (xy 13.97 8.89)
          (xy 7.62 12.7)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 20.32 17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 5.08 9.144) (end 6.35 8.636)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin input line (at 27.94 13.97 180) (length 7.62)
        (name "CON" (effects (font (size 1.524 1.524))))
        (number "1" (effects (font (size 1.524 1.524))))
      )
      (pin power_in line (at -7.62 3.81 0) (length 7.62)
        (name "VSS" (effects (font (size 1.524 1.524))))
        (number "2" (effects (font (size 1.524 1.524))))
      )
      (pin output line (at 27.94 8.89 180) (length 7.62)
        (name "OUT" (effects (font (size 1.524 1.524))))
        (number "3" (effects (font (size 1.524 1.524))))
      )
      (pin power_in line (at -7.62 13.97 0) (length 7.62)
        (name "VDD" (effects (font (size 1.524 1.524))))
        (number "4" (effects (font (size 1.524 1.524))))
      )
    )
  )
  (symbol "PI6CV304" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0.508 1.016 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PI6CV304" (id 1) (at 8.89 -5.588 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/115/PI6CV304-1536456.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "140/160 MHz clock buffer" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PI6CV304_0_1"
      (polyline
        (pts
          (xy 0 -24.13)
          (xy 11.43 -24.13)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.508 -26.67)
          (xy 0 -26.67)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -28.194)
          (xy 12.7 -26.67)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -26.67)
          (xy 0.508 -26.67)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -23.114)
          (xy 12.7 -21.59)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -21.59)
          (xy 4.572 -21.59)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -16.51)
          (xy 4.572 -16.51)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -24.13)
          (xy 11.43 -25.908)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -19.05)
          (xy 8.128 -19.05)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -19.05)
          (xy 11.43 -20.828)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -13.97)
          (xy 8.128 -13.97)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 -26.67)
          (xy 12.7 -26.67)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 -21.59)
          (xy 12.7 -21.59)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.572 -26.67)
          (xy 4.572 -11.43)
          (xy 10.16 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.128 -24.13)
          (xy 8.128 -8.89)
          (xy 11.43 -8.89)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -28.194)
          (xy 10.16 -25.146)
          (xy 12.7 -26.67)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -23.114)
          (xy 10.16 -20.066)
          (xy 12.7 -21.59)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 17.78 -29.21)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle (center 4.572 -26.67) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 4.572 -21.59) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 4.572 -16.51) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 8.128 -24.13) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 8.128 -19.05) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 8.128 -13.97) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
    )
    (symbol "PI6CV304_1_1"
      (polyline
        (pts
          (xy 10.16 -18.034)
          (xy 12.7 -16.51)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -12.954)
          (xy 12.7 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -13.97)
          (xy 11.43 -15.748)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -8.89)
          (xy 11.43 -10.668)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 -16.51)
          (xy 12.7 -16.51)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 -11.43)
          (xy 12.7 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -18.034)
          (xy 10.16 -14.986)
          (xy 12.7 -16.51)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -12.954)
          (xy 10.16 -9.906)
          (xy 12.7 -11.43)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin input clock (at -5.08 -26.67 0) (length 5.08)
        (name "CLK_IN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -24.13 0) (length 5.08)
        (name "OE" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -11.43 180) (length 5.08)
        (name "Y0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -1.27 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -16.51 180) (length 5.08)
        (name "Y1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -1.27 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -21.59 180) (length 5.08)
        (name "Y2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -26.67 180) (length 5.08)
        (name "Y3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PI6CV2304" (extends "PI6CV304")
    (property "Reference" "U" (id 0) (at 0.508 1.016 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PI6CV2304" (id 1) (at 8.89 -5.588 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/115/PI6CV304-1536456.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "140 MHz clock buffer" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "SG5032VAN" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SG5032VAN" (id 1) (at 8.89 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SG5032VAN_0_1"
      (rectangle (start 0 0) (end 13.97 -12.7)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SG5032VAN_1_1"
      (pin input line (at -2.54 -6.35 0) (length 2.54)
        (name "OE" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 -5.08 180) (length 2.54)
        (name "OUT+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 -7.62 180) (length 2.54)
        (name "OUT-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -2.54 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Si53306-B-GM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 16.51 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Si53306-B-GM" (id 1) (at 22.86 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Si53306-B-GM_0_1"
      (rectangle (start 0 0) (end 20.32 -33.02)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "Si53306-B-GM_1_1"
      (pin power_in line (at 8.89 5.08 270) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -19.05 180) (length 5.08)
        (name "Q2+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -15.24 180) (length 5.08)
        (name "Q1-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -12.7 180) (length 5.08)
        (name "Q1+" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -22.86 0) (length 5.08)
        (name "SFOUT0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -8.89 180) (length 5.08)
        (name "Q0-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -6.35 180) (length 5.08)
        (name "Q0+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "OE" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -38.1 90) (length 5.08)
        (name "GNDPAD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -5.08 -12.7 0) (length 5.08)
        (name "CLK+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -5.08 -15.24 0) (length 5.08)
        (name "CLK-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 -38.1 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 5.08 270) (length 5.08)
        (name "VDDO" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -27.94 180) (length 5.08)
        (name "Q3-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -25.4 180) (length 5.08)
        (name "Q3+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -25.4 0) (length 5.08)
        (name "SFOUT1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -21.59 180) (length 5.08)
        (name "Q2-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
