(module NINIGI-TSM1XXC3 (layer F.Cu) (tedit 600D857B)
  (fp_text reference REF** (at -4.3 -3.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NINIGI-TSM1XXC3 (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -6.6) (end 10 -6.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 10 -6.6) (end 10 6.6) (layer F.SilkS) (width 0.3))
  (fp_line (start 10 6.6) (end 0 6.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 6.6) (end 0 4.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 4.4) (end 0 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -6.6) (end 0 -4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 10 -4.7) (end 11 -4.7) (layer F.SilkS) (width 0.3))
  (fp_line (start 10 0) (end 11 0) (layer F.SilkS) (width 0.3))
  (fp_line (start 10 4.7) (end 11.1 4.7) (layer F.SilkS) (width 0.3))
  (fp_line (start 0 -6.6) (end 10 -6.6) (layer F.Fab) (width 0.12))
  (fp_line (start 10 -6.6) (end 10 6.6) (layer F.Fab) (width 0.12))
  (fp_line (start 10 6.6) (end 0 6.6) (layer F.Fab) (width 0.12))
  (fp_line (start 0 6.6) (end 0 -6.6) (layer F.Fab) (width 0.12))
  (fp_line (start 10 0.6) (end 11.1 0.6) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 0.6) (end 11.1 -0.6) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 -0.6) (end 10 -0.6) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 4.1) (end 10 4.1) (layer F.Fab) (width 0.12))
  (fp_line (start 10 5.3) (end 11.1 5.3) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 5.3) (end 11.1 4.1) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 -5.3) (end 10 -5.3) (layer F.Fab) (width 0.12))
  (fp_line (start 10 -4.1) (end 11.1 -4.1) (layer F.Fab) (width 0.12))
  (fp_line (start 11.1 -4.1) (end 11.1 -5.3) (layer F.Fab) (width 0.12))
  (fp_line (start 0 3) (end -7.3 3) (layer F.Fab) (width 0.12))
  (fp_line (start -7.3 3) (end -7.3 -3) (layer F.Fab) (width 0.12))
  (fp_line (start -7.3 -3) (end 0 -3) (layer F.Fab) (width 0.12))
  (fp_line (start -7.3 -0.8) (end -12.9 -3) (layer F.Fab) (width 0.12))
  (fp_line (start -12.9 -3) (end -13.8 -1.6) (layer F.Fab) (width 0.12))
  (fp_line (start -13.8 -1.6) (end -7.3 0.9) (layer F.Fab) (width 0.12))
  (pad MP thru_hole circle (at 0 -2.5) (size 3 3) (drill 1.9) (layers *.Cu *.Mask))
  (pad MP thru_hole circle (at 0 2.5) (size 3 3) (drill 1.9) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 12.7 -4.7) (size 3 3) (drill 1.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 12.7 0) (size 3 3) (drill 1.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 12.7 4.7) (size 3 3) (drill 1.9) (layers *.Cu *.Mask))
)
