(module PulseElectronics_PA4332 (layer F.Cu) (tedit 60FC0F21)
  (fp_text reference REF** (at 0 -6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PulseElectronics_PA4332 (at 0 -3.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.75 -2.1) (end 1.75 -2.1) (layer F.Fab) (width 0.12))
  (fp_line (start 2.1 -1.75) (end 2.1 1.75) (layer F.Fab) (width 0.12))
  (fp_line (start 1.75 2.1) (end -1.75 2.1) (layer F.Fab) (width 0.12))
  (fp_line (start -2.1 1.75) (end -2.1 -1.75) (layer F.Fab) (width 0.12))
  (fp_line (start -2.1 -1.75) (end -1.75 -2.1) (layer F.Fab) (width 0.12))
  (fp_line (start 1.75 -2.1) (end 2.1 -1.75) (layer F.Fab) (width 0.12))
  (fp_line (start 2.1 1.75) (end 1.75 2.1) (layer F.Fab) (width 0.12))
  (fp_line (start -2.1 1.75) (end -1.75 2.1) (layer F.Fab) (width 0.12))
  (fp_line (start -2.25 -2.25) (end 2.25 -2.25) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 -2.25) (end 2.25 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 -2.25) (end -2.25 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 2) (end -2.25 2.25) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 2.25) (end 2.25 2.25) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 2.25) (end 2.25 2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 -2.25) (end 2.25 -2.25) (layer F.CrtYd) (width 0.12))
  (fp_line (start 2.25 -2.25) (end 2.25 2.25) (layer F.CrtYd) (width 0.12))
  (fp_line (start 2.25 2.25) (end -2.25 2.25) (layer F.CrtYd) (width 0.12))
  (fp_line (start -2.25 2.25) (end -2.25 -2.25) (layer F.CrtYd) (width 0.12))
  (pad 1 smd rect (at -1.5 0) (size 1.1 3.7) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.5 0) (size 1.1 3.7) (layers F.Cu F.Paste F.Mask))
)
