(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "STM32F407VGT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "STM32F407VGT" (id 1) (at 8.89 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -12.7 12.7 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at -12.7 12.7 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "STM32F407VGT_1_1"
      (rectangle (start 0 0) (end 12.7 -34.29)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 17.78 -2.54 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "100" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -19.05 180) (length 5.08)
        (name "VSSA" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -21.59 0) (length 5.08)
        (name "VREF+" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -19.05 0) (length 5.08)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -5.08 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -25.4 0) (length 5.08)
        (name "VCAP1" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -31.75 0) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -27.94 0) (length 5.08)
        (name "VCAP2" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -7.62 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -10.16 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "99" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_2_0"
      (text "Port A" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407VGT_2_1"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PA0_WKUP" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PA13_JTMS_SWDIO" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PA14_JTCK_SWCLK" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PA15_JTDI" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_3_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port B" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407VGT_3_1"
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -7.62 0) (length 5.08)
        (name "PB2_BOOT1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PB3_JTDO_TRCSWO" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PB4_NJTRST" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "91" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "92" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "93" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "95" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "96" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_4_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port C" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407VGT_4_1"
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PC8" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PC9" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PC13" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PC10" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PC11" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -38.1 0) (length 5.08)
        (name "PC14_OSC32_IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PC12" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -40.64 0) (length 5.08)
        (name "PC15_OSC32_IN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_5_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port D" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407VGT_5_1"
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PD8" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PD9" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PD10" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PD11" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PD12" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PD13" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PD14" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PD15" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_6_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port E" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407VGT_6_1"
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PE2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PE3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PE4" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PE7" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PE8" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PE5" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PE9" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PE10" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PE11" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PE12" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PE13" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PE14" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PE15" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PE6" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "PE0" (effects (font (size 1.27 1.27))))
        (number "97" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "PE1" (effects (font (size 1.27 1.27))))
        (number "98" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407VGT_7_0"
      (rectangle (start 0 0) (end 13.97 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "STM32F407VGT_7_1"
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PH0_OSCIN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PH1_OSCOUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -8.89 0) (length 5.08)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -11.43 0) (length 5.08)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "94" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "STM32F407ZGT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "STM32F407ZGT" (id 1) (at 8.89 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -12.7 12.7 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/ef/92/76/6d/bb/c2/4f/f7/DM00037051.pdf/files/DM00037051.pdf/jcr:content/translations/en.DM00037051.pdf" (id 3) (at -12.7 12.7 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "STM32 ARM Microcontroller Controller" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ARM Cortex-M4 32b MCU+FPU, 210DMIPS, up to 1MB Flash/192+4KB RAM, USB OTG HS/FS, Ethernet, 17 TIMs, 3 ADCs, 15 comm. interfaces & camera" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LQFP144 LQFP-144" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM32F407ZGT_1_1"
      (rectangle (start 0 0) (end 15.24 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 20.32 -33.02 180) (length 5.08)
        (name "VCAP2" (effects (font (size 1.27 1.27))))
        (number "106" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -17.78 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "107" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -22.86 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "108" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -20.32 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "120" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -25.4 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "121" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -22.86 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "130" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -27.94 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "131" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -30.48 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "144" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -2.54 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -26.67 180) (length 5.08)
        (name "VSSA" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -36.83 0) (length 5.08)
        (name "VREF+" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -34.29 0) (length 5.08)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -5.08 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -7.62 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -40.64 0) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -10.16 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -30.48 180) (length 5.08)
        (name "VCAP1" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -12.7 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -17.78 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -15.24 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "94" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -20.32 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "95" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_2_0"
      (text "Port A" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407ZGT_2_1"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "100" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "101" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "102" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "103" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "104" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PA13/JTMS/SWDIO" (effects (font (size 1.27 1.27))))
        (number "105" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PA14/JTCK/SWCLK" (effects (font (size 1.27 1.27))))
        (number "109" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PA15/JTDI" (effects (font (size 1.27 1.27))))
        (number "110" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PA0/WKUP" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_3_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port B" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407ZGT_3_1"
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PB3/JTDO/TCSWO" (effects (font (size 1.27 1.27))))
        (number "133" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PB4/NJRST" (effects (font (size 1.27 1.27))))
        (number "134" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "135" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "136" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "137" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "139" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "140" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PB2/BOOT1" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_4_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port C" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407ZGT_4_1"
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PC10" (effects (font (size 1.27 1.27))))
        (number "111" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PC11" (effects (font (size 1.27 1.27))))
        (number "112" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PC12" (effects (font (size 1.27 1.27))))
        (number "113" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PC13" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PC14/OSC32_IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PC15/OSC32_OUT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "96" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "97" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PC8" (effects (font (size 1.27 1.27))))
        (number "98" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PC9" (effects (font (size 1.27 1.27))))
        (number "99" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_5_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port D" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407ZGT_5_1"
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "114" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "115" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "116" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "117" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "118" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "119" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "122" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "123" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PD8" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PD9" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PD10" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PD11" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PD12" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PD13" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PD14" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PD15" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_6_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port E" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
    )
    (symbol "STM32F407ZGT_6_1"
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PE2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PE0" (effects (font (size 1.27 1.27))))
        (number "141" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PE1" (effects (font (size 1.27 1.27))))
        (number "142" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PE3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PE4" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PE5" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PE6" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PE7" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PE8" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PE9" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PE10" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PE11" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PE12" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PE13" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PE14" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PE15" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_7_0"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "STM32F407ZGT_7_1"
      (text "Port F" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PF0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PF1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PF2" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PF3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PF4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PF5" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PF6" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PF7" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PF8" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PF9" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PF10" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PF11" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PF12" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PF13" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PF14" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PF15" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_8_1"
      (rectangle (start 0 0) (end 19.05 -43.18)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Port G" (at 11.43 -20.32 900)
        (effects (font (size 1.524 1.524)))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PG9" (effects (font (size 1.27 1.27))))
        (number "124" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PG10" (effects (font (size 1.27 1.27))))
        (number "125" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PG11" (effects (font (size 1.27 1.27))))
        (number "126" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PG12" (effects (font (size 1.27 1.27))))
        (number "127" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PG13" (effects (font (size 1.27 1.27))))
        (number "128" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PG14" (effects (font (size 1.27 1.27))))
        (number "129" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PG15" (effects (font (size 1.27 1.27))))
        (number "132" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PG0" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PG1" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PG2" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PG3" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PG4" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PG5" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PG6" (effects (font (size 1.27 1.27))))
        (number "91" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PG7" (effects (font (size 1.27 1.27))))
        (number "92" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PG8" (effects (font (size 1.27 1.27))))
        (number "93" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STM32F407ZGT_9_1"
      (rectangle (start 0 0) (end 19.05 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -5.08 -12.7 0) (length 5.08)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "138" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -15.24 0) (length 5.08)
        (name "PDR_ON" (effects (font (size 1.27 1.27))))
        (number "143" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "PH0/OSC_IN" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PH1/OSC_OUT" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -10.16 0) (length 5.08)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "STM32G473CxU" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "STM32G473CxU" (id 1) (at 20.32 -26.67 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "STM32F743 Controller in QFN 48 package" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM32G473CxU_0_1"
      (rectangle (start 0 0) (end 38.1 -60.96)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "STM32G473CxU_1_1"
      (pin power_in line (at 25.4 5.08 270) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -44.45 180) (length 5.08)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -2.54 180) (length 5.08)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -5.08 180) (length 5.08)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -7.62 180) (length 5.08)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -54.61 180) (length 5.08)
        (name "PC13" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 30.48 5.08 270) (length 5.08)
        (name "VREF+" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 5.08 270) (length 5.08)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -27.94 180) (length 5.08)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.24 5.08 270) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -30.48 180) (length 5.08)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -33.02 180) (length 5.08)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -35.56 180) (length 5.08)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -38.1 180) (length 5.08)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -40.64 180) (length 5.08)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -46.99 180) (length 5.08)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -57.15 180) (length 5.08)
        (name "PC14-OSC32IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -30.48 0) (length 5.08)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -33.02 0) (length 5.08)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -35.56 0) (length 5.08)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -38.1 0) (length 5.08)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 5.08 270) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -40.64 0) (length 5.08)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -43.18 0) (length 5.08)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -45.72 0) (length 5.08)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -49.53 180) (length 5.08)
        (name "PC10" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -59.69 180) (length 5.08)
        (name "PC15-OSC32OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -52.07 180) (length 5.08)
        (name "PC11" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -10.16 180) (length 5.08)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -12.7 180) (length 5.08)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -15.24 180) (length 5.08)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -17.78 180) (length 5.08)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -20.32 180) (length 5.08)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -22.86 180) (length 5.08)
        (name "PB8-BOOT0" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -25.4 180) (length 5.08)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 5.08 270) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 -66.04 90) (length 5.08)
        (name "VSS-PAD" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -55.88 0) (length 5.08)
        (name "PF0-OSCIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -58.42 0) (length 5.08)
        (name "PF1-OSCOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -3.81 0) (length 5.08)
        (name "PG10-~{NRST}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
