EESchema-DOCLIB  Version 2.0
#
$CMP FT4232HQ
D Hi Speed Quad Channel USB UART/FIFO, LQFP/QFN-64
K FTDI USB Quad UART FIFO
F https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4232H.pdf
$ENDCMP
#
$CMP KSZ8081RND
D 10BASE-T/100BASE-TX PHY with RMII Support, 50 MHz input clock, QFN-24
K ETH PHY RMII
F http://ww1.microchip.com/downloads/en/DeviceDoc/00002199A.pdf
$ENDCMP
#
$CMP KSZ8091RNA
D 10BASE-T/100BASE-TX PHY with RMII Support, 25 MHz input clock/50 MHz output, QFN-24
K ETH PHY RMII
F http://ww1.microchip.com/downloads/en/DeviceDoc/00002199A.pdf
$ENDCMP
#
$CMP KSZ8091RND
D 10BASE-T/100BASE-TX PHY with RMII Support, 50 MHz input clock, QFN-24
K ETH PHY RMII
F https://www.mouser.de/datasheet/2/268/00002298A-1890829.pdf
$ENDCMP
#
$CMP ST3485E
D 3.3 V powered, 15 kV ESD protected, up to 12 Mbps RS-485/RS-422 transceiver
K RS422,RS485
F https://www.st.com/resource/en/datasheet/st3485ec.pdf
$ENDCMP
#
#End Doc Library
