(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "10PIN_JTAG_SWD" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -7.112 1.016 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "10PIN_JTAG_SWD" (id 1) (at 0.254 2.794 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "10PIN_JTAG_SWD_0_1"
      (rectangle (start -20.828 0) (end 0 -25.4)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "10PIN_JTAG_SWD_1_1"
      (pin passive line (at 2.54 -1.27 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -8.89 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -11.43 180) (length 2.54)
        (name "TMS/SWDIO" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -6.35 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -13.97 180) (length 2.54)
        (name "TCK/SWCLK" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -3.81 180) (length 2.54)
        (name "TESTMODE/VCC/GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -16.51 180) (length 2.54)
        (name "TDO/SWO" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -21.59 180) (length 2.54)
        (name "RX/RTCLK" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -19.05 180) (length 2.54)
        (name "TDI" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -24.13 180) (length 2.54)
        (name "TX/~{TRST}" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "16Pin_Text_LCD" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.842 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "16Pin_Text_LCD" (id 1) (at 3.81 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Display:RC1602A" (id 2) (at 0 -22.86 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.raystar-optronics.com/down.php?ProID=18" (id 3) (at -12.7 17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "display LCD dot-matrix" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LCD 16x2 Alphanumeric 16pin Gray Backlight" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RC1602A*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "16Pin_Text_LCD_0_0"
      (rectangle (start -2.794 8.89) (end 3.81 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "16x2" (at 0.254 6.35 0)
        (effects (font (size 0.9906 0.9906) bold))
      )
    )
    (symbol "16Pin_Text_LCD_0_1"
      (rectangle (start -7.62 17.78) (end 7.62 -17.78)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "16Pin_Text_LCD_1_1"
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -5.08 0) (length 2.54)
        (name "DB3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -7.62 0) (length 2.54)
        (name "DB4" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
        (name "DB5" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -12.7 0) (length 2.54)
        (name "DB6" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -15.24 0) (length 2.54)
        (name "DB7" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "A/VEE" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 2.54 180) (length 2.54)
        (name "K" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "Vo" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "RS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "R/~{W}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "~{E}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
        (name "DB0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 0 0) (length 2.54)
        (name "DB1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "DB2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HDMI-Jack" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "P" (id 0) (at 15.24 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "HDMI-Jack" (id 1) (at 6.35 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_description" "HDMI Jack" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HDMI-Jack_0_1"
      (rectangle (start 0 0) (end 22.86 -63.5)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "HDMI-Jack_1_1"
      (pin input line (at -5.08 -15.24 0) (length 5.08)
        (name "TMDS2+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -21.59 0) (length 5.08)
        (name "TMDSC+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -62.23 0) (length 5.08)
        (name "TMDSCS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -24.13 0) (length 5.08)
        (name "TMDSC-" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -33.02 0) (length 5.08)
        (name "CEC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -49.53 0) (length 5.08)
        (name "ETH/AUDRET/RESV" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -45.72 0) (length 5.08)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -43.18 0) (length 5.08)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -40.64 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -38.1 0) (length 5.08)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -35.56 0) (length 5.08)
        (name "HOTPLUG" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -59.69 0) (length 5.08)
        (name "TMDS2S" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -11.43 180) (length 5.08)
        (name "HOUSING" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -8.89 180) (length 5.08)
        (name "HOUSING" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -6.35 180) (length 5.08)
        (name "HOUSING" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -3.81 180) (length 5.08)
        (name "HOUSING" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -17.78 0) (length 5.08)
        (name "TMDS2-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -8.89 0) (length 5.08)
        (name "TMDS1+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -57.15 0) (length 5.08)
        (name "TMDS1S" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -11.43 0) (length 5.08)
        (name "TMDS1-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -2.54 0) (length 5.08)
        (name "TMDS0+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -54.61 0) (length 5.08)
        (name "TMDS0S" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "TMDS0-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "JACK_TRS_3PINS" (pin_names (offset 0.762)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -8.89 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "JACK_TRS_3PINS" (id 1) (at -1.27 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 2.54 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Datasheet" "" (id 3) (at 2.54 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "JACK_TRS_3PINS_0_0"
      (polyline
        (pts
          (xy -8.89 3.81)
          (xy -7.62 2.54)
          (xy -6.35 3.81)
          (xy 7.62 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -6.35 0.762)
          (xy -5.08 2.032)
          (xy -1.778 -1.27)
          (xy 7.62 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "JACK_TRS_3PINS_0_1"
      (rectangle (start -11.43 3.81) (end -10.16 -1.27)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 0.762 1.27)
          (xy 7.62 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 1.27)
          (xy 0 2.032)
          (xy -0.762 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 7.62 -3.81) (end -10.16 6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "JACK_TRS_3PINS_1_1"
      (pin passive line (at 10.16 3.81 180) (length 2.54)
        (name "S" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 1.27 180) (length 2.54)
        (name "T" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -1.27 180) (length 2.54)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Micro_SD" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "CON" (id 0) (at 46.99 13.97 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "Micro_SD" (id 1) (at 31.75 27.94 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "Micro_SD_0_1"
      (polyline
        (pts
          (xy 6.35 44.45)
          (xy 6.35 24.13)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 44.45)
          (xy 36.83 44.45)
          (xy 38.1 43.18)
          (xy 38.1 26.67)
          (xy 36.83 25.4)
          (xy 29.21 25.4)
          (xy 27.94 24.13)
          (xy 22.86 24.13)
          (xy 21.59 25.4)
          (xy 20.32 25.4)
          (xy 19.05 24.13)
          (xy 5.08 24.13)
          (xy 5.08 44.45)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 48.26 52.07) (end 8.89 16.51)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Micro_SD_1_1"
      (pin input line (at 53.34 25.4 180) (length 5.08)
        (name "DAT2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 31.75 11.43 90) (length 5.08)
        (name "SHELL" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 11.43 90) (length 5.08)
        (name "SHELL" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 57.15 270) (length 5.08)
        (name "SHELL" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 31.75 57.15 270) (length 5.08)
        (name "SHELL" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 27.94 180) (length 5.08)
        (name "CD/DAT3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 30.48 180) (length 5.08)
        (name "CMD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 33.02 180) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 35.56 180) (length 5.08)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 38.1 180) (length 5.08)
        (name "GND/VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 40.64 180) (length 5.08)
        (name "DAT0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 43.18 180) (length 5.08)
        (name "DAT1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 53.34 48.26 180) (length 5.08)
        (name "CARD_DETECT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Rotary_Encoder_Switch_Mounting" (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (id 0) (at 0 6.604 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Rotary_Encoder_Switch_Mounting" (id 1) (at 0 -6.604 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at -3.81 4.064 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 0 6.604 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "rotary switch encoder switch push button" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RotaryEncoder*Switch*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Rotary_Encoder_Switch_Mounting_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle (center -3.81 0) (radius 0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (arc (start -0.381 -2.794) (mid 2.3622 -0.0508) (end -0.381 2.667)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center -0.381 0) (radius 1.905)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -1.778)
          (xy -0.635 1.778)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.381 -1.778)
          (xy -0.381 1.778)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.127 1.778)
          (xy -0.127 -1.778)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 0)
          (xy 3.429 0)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 1.016)
          (xy 3.81 -1.016)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -2.54)
          (xy -3.81 -2.54)
          (xy -3.81 -2.032)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54)
          (xy -3.81 2.54)
          (xy -3.81 2.032)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.254 -3.048)
          (xy -0.508 -2.794)
          (xy 0.127 -2.413)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.254 2.921)
          (xy -0.508 2.667)
          (xy 0.127 2.286)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -2.54)
          (xy 4.318 -2.54)
          (xy 4.318 -1.016)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 4.318 2.54)
          (xy 4.318 1.016)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 0)
          (xy -3.81 0)
          (xy -3.81 -1.016)
          (xy -3.302 -2.032)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -4.318 0)
          (xy -3.81 0)
          (xy -3.81 1.016)
          (xy -3.302 2.032)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 4.318 -1.016) (radius 0.127)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle (center 4.318 1.016) (radius 0.127)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Rotary_Encoder_Switch_Mounting_1_1"
      (pin passive line (at -7.62 2.54 0) (length 2.54)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "A" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -2.54 0) (length 2.54)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "B" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "C" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 2.54)
        (name "MP" (effects (font (size 1.27 1.27))))
        (number "MP" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 2.54 180) (length 2.54)
        (name "S1" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -2.54 180) (length 2.54)
        (name "S2" (effects (font (size 1.27 1.27))))
        (number "S2" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
