(module Bosch_LGA-16_4.5x3mm_P0.5mm_ClockwisePinNumbering (layer F.Cu) (tedit 5DC9E3DC)
  (attr smd)
  (fp_text reference REF** (at 0.2 -2.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Bosch_LGA-16_4.5x3mm_P0.5mm_ClockwisePinNumbering (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.5 -1.7) (end -2.15 -1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5 1.7) (end 2.5 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5 -1.35) (end -2.5 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.5 -1.7) (end 2.5 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.15 -1.7) (end -2.5 -1.35) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -2.05 -1.5) (xy -2.3 -1.25) (xy -2.3 -0.8) (xy -1.8 -0.8)
    (xy -1.8 -1.5)) (layer Eco1.User) (width 0.1))
  (pad 1 smd roundrect (at -1.5 -1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1 -1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.5 -1.165 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0 -1.165 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.5 -1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1 -1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 1.5 -1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0 1.165 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -1 1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -0.5 1.165 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 1.5 1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 1 1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -1.5 1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 0.5 1.165) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.915 0 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -1.915 0 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/smd.shapes3d/Bosch_LGA-16_4.5x3mm_P0.5mm_ClockwisePinNumbering.x3d
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
