(module Micro_SD_Amphenol (layer F.Cu) (tedit 568E8254)
  (fp_text reference REF** (at -16.51 16.51) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Micro_SD_Amphenol (at -15.24 19.05) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 3.81) (end 0 -7.62) (layer F.Adhes) (width 0.15))
  (fp_line (start 8.89 3.81) (end 0 3.81) (layer F.Adhes) (width 0.15))
  (fp_line (start 8.89 -2.54) (end 8.89 3.81) (layer F.Adhes) (width 0.15))
  (fp_line (start 7.62 -3.81) (end 8.89 -2.54) (layer F.Adhes) (width 0.15))
  (fp_line (start 7.62 -7.62) (end 7.62 -3.81) (layer F.Adhes) (width 0.15))
  (fp_line (start 0 -7.62) (end 7.62 -7.62) (layer F.Adhes) (width 0.15))
  (fp_text user SD_CARD (at 3.81 -2.54) (layer F.Adhes)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.45 -10.25) (end -1.45 1.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.45 1.2) (end 10.5 1.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.5 1.2) (end 10.5 -10.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.5 -10.25) (end -1.45 -10.25) (layer F.SilkS) (width 0.15))
  (pad 10 smd rect (at 10.23 -9.925) (size 1 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 10.5 -7.5) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.45 -6.85) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.125 -8.35) (size 1.45 1) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 10.15 0.75) (size 1.5 1.5) (layers F.Cu F.Paste B.SilkS F.Mask))
  (pad 8 smd rect (at 0 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.1 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.2 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.3 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 4.4 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 5.5 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 6.6 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 7.7 0.875) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.2 0.75) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask))
)
