(module Oscillator-SMD (layer F.Cu) (tedit 56D83549)
  (descr http://www.tme.eu/en/Document/04fa0ef07f38450711886bdf482cf79c/ISM92_Series.pdf)
  (tags "SMD Ceramic Crystal Oscillator HC-MOS")
  (fp_text reference REF** (at 1 1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Oscillator-SMD (at 4.4 3.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.9 0.8) (end -0.6 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.9 0.5) (end -0.9 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.9 -2.8) (end -1 -2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -2.8) (end 0.9 -2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.9 -2.8) (end 3.8 -2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.9 0.3) (end 3.8 0.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.9 0.3) (end 2 0.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.3) (end -1 -2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.9 0.3) (end -1 0.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.9 -2.8) (end 3.9 0.3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at 0 0) (size 1.6 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.9 0) (size 1.6 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.9 -2.5) (size 1.6 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 -2.5) (size 1.6 1.35) (layers F.Cu F.Paste F.Mask))
)
