(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "LCMXO2-1200HC-4SG32C" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 10.16 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LCMXO2-1200HC-4SG32C" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "http://www.latticesemi.com/~/media/LatticeSemi/Documents/DataSheets/MachXO23/MachXO2FamilyDataSheet.pdf?document_id=38834" (id 3) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Lattice MachXO2 FPGA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Lattice MachXO2 FPGA" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN32 QFN-32" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LCMXO2-1200HC-4SG32C_1_1"
      (rectangle (start 0 -2.54) (end 20.32 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 0) (end 20.32 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "FPGA Power" (at 10.16 -1.27 0)
        (effects (font (size 1.524 1.524)))
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -7.62 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -5.08 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at -5.08 -11.43 0) (length 5.08)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LCMXO2-1200HC-4SG32C_2_1"
      (rectangle (start 0 -2.54) (end 20.32 -34.29)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 20.32 0) (end 0 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Bank 0" (at 10.16 -1.27 0)
        (effects (font (size 1.524 1.524)))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PT10C_TDO" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PT17D_DONE" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -29.21 0) (length 5.08)
        (name "VCCIO0" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional inverted (at -5.08 -5.08 0) (length 5.08)
        (name "PT15D_PROGRAMN" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PT15C_JTAGENB" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PT12D_SDAPCLKC0" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PT12C_SCLPCLKT0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PT11D_TMS" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PT11C_TCK" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -31.75 0) (length 5.08)
        (name "VCCIO0" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PT10D_TDI" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LCMXO2-1200HC-4SG32C_3_1"
      (rectangle (start 0 -2.54) (end 20.32 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 0) (end 20.32 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Bank 1" (at 10.16 -1.27 0)
        (effects (font (size 1.524 1.524)))
      )
      (pin power_in line (at -5.08 -11.43 0) (length 5.08)
        (name "VCCIO1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PR5D_PCLKC1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PR5C_PCLKT1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LCMXO2-1200HC-4SG32C_4_1"
      (rectangle (start 0 -2.54) (end 20.32 -34.29)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 0) (end 20.32 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Bank 2" (at 10.16 -1.27 0)
        (effects (font (size 1.524 1.524)))
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "PB6D_SOSPISO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "PB9A_PCLKT20" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "PB9B_PCLKC20" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "PB11A_PCLKT21" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "PB11B_PCLKC21" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -29.21 0) (length 5.08)
        (name "VCCIO2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "PB20C_SN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -25.4 0) (length 5.08)
        (name "PB20D_SISPI" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -31.75 0) (length 5.08)
        (name "VCCIO2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PB4C_CSSPIN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PB6C_MCLKCCLK" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LCMXO2-1200HC-4SG32C_5_1"
      (rectangle (start 0 -2.54) (end 20.32 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 0) (end 20.32 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "Bank 3" (at 10.16 -1.27 0)
        (effects (font (size 1.524 1.524)))
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "PL9A_PCLKT3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "PL9B_PCLKC3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -11.43 0) (length 5.08)
        (name "VCCIO3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LCMXO2-1200HC-5SG32C" (extends "LCMXO2-1200HC-4SG32C")
    (property "Reference" "U" (id 0) (at 10.16 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LCMXO2-1200HC-5SG32C" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_keywords" "Lattice MachXO2 FPGA" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Lattice MachXO2 FPGA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN32 QFN-32" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "LCMXO2-1200HC-6SG32C" (extends "LCMXO2-1200HC-4SG32C")
    (property "Reference" "U" (id 0) (at 10.16 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LCMXO2-1200HC-6SG32C" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 6.35 -17.78 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_keywords" "Lattice MachXO2 FPGA" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Lattice MachXO2 FPGA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN32 QFN-32" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "LFXP2-5E-6TN144C" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 22.86 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LFXP2-5E-6TN144C" (id 1) (at 0 20.32 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -17.78 8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "http://www.latticesemi.com/en/Products/FPGAandCPLD/LatticeXP2.aspx" (id 3) (at -26.67 31.75 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Version" "1.0" (id 4) (at -92.71 29.21 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Author" "Makise Kurisu <kurisu@shimatta.de>" (id 5) (at -72.39 26.67 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_locked" "" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Lattice XP2 FPGA PLD" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Lattice XP2-5E FPGA (TQFP144, Speedgrade -6)" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TQFP-144" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LFXP2-5E-6TN144C_1_1"
      (rectangle (start 11.43 19.05) (end -11.43 -19.05)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -16.51 -3.81 0) (length 5.08)
        (name "VCCAUX4" (effects (font (size 1.27 1.27))))
        (number "117" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 8.89 0) (length 5.08)
        (name "VCC4" (effects (font (size 1.27 1.27))))
        (number "118" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -16.51 0) (length 5.08)
        (name "ULC_GNDPLL" (effects (font (size 1.27 1.27))))
        (number "139" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -13.97 0) (length 5.08)
        (name "ULC_VCCPLL" (effects (font (size 1.27 1.27))))
        (number "140" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 3.81 0) (length 5.08)
        (name "VCCAUX1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 16.51 0) (length 5.08)
        (name "VCC1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 1.27 180) (length 5.08)
        (name "TOE" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -1.27 180) (length 5.08)
        (name "CFG0" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 13.97 0) (length 5.08)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 1.27 0) (length 5.08)
        (name "VCCAUX2" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -8.89 0) (length 5.08)
        (name "LRC_VCCPLL" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -11.43 0) (length 5.08)
        (name "LRC_GNDPLL" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 11.43 0) (length 5.08)
        (name "VCC3" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -1.27 0) (length 5.08)
        (name "VCCAUX3" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 16.51 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LFXP2-5E-6TN144C_2_0"
      (text "BANK0" (at 6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
      (text "BANK1" (at -6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
    )
    (symbol "LFXP2-5E-6TN144C_2_1"
      (rectangle (start 11.43 19.05) (end -11.43 -53.34)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -16.51 12.7 0) (length 5.08)
        (name "PT28B" (effects (font (size 1.27 1.27))))
        (number "109" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 10.16 0) (length 5.08)
        (name "PT28A" (effects (font (size 1.27 1.27))))
        (number "110" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -50.8 0) (length 5.08)
        (name "GNDIO1" (effects (font (size 1.27 1.27))))
        (number "111" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -48.26 0) (length 5.08)
        (name "VCCIO1" (effects (font (size 1.27 1.27))))
        (number "112" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 7.62 0) (length 5.08)
        (name "PT21B" (effects (font (size 1.27 1.27))))
        (number "113" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 5.08 0) (length 5.08)
        (name "PT20B" (effects (font (size 1.27 1.27))))
        (number "114" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 2.54 0) (length 5.08)
        (name "PT21A" (effects (font (size 1.27 1.27))))
        (number "115" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 0 0) (length 5.08)
        (name "PT20A" (effects (font (size 1.27 1.27))))
        (number "116" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 12.7 180) (length 5.08)
        (name "PT19B" (effects (font (size 1.27 1.27))))
        (number "119" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 10.16 180) (length 5.08)
        (name "PT19A" (effects (font (size 1.27 1.27))))
        (number "120" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 7.62 180) (length 5.08)
        (name "PT18B" (effects (font (size 1.27 1.27))))
        (number "121" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 5.08 180) (length 5.08)
        (name "PT17B" (effects (font (size 1.27 1.27))))
        (number "122" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 2.54 180) (length 5.08)
        (name "PT18A" (effects (font (size 1.27 1.27))))
        (number "123" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 0 180) (length 5.08)
        (name "PT17A" (effects (font (size 1.27 1.27))))
        (number "124" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -2.54 180) (length 5.08)
        (name "PT16B" (effects (font (size 1.27 1.27))))
        (number "125" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -48.26 180) (length 5.08)
        (name "GNDIO01" (effects (font (size 1.27 1.27))))
        (number "126" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -5.08 180) (length 5.08)
        (name "PT16A" (effects (font (size 1.27 1.27))))
        (number "127" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -43.18 180) (length 5.08)
        (name "VCCIO01" (effects (font (size 1.27 1.27))))
        (number "128" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -7.62 180) (length 5.08)
        (name "PT15B" (effects (font (size 1.27 1.27))))
        (number "129" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -10.16 180) (length 5.08)
        (name "PT14B" (effects (font (size 1.27 1.27))))
        (number "130" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -12.7 180) (length 5.08)
        (name "PT15A" (effects (font (size 1.27 1.27))))
        (number "131" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -15.24 180) (length 5.08)
        (name "PT14A" (effects (font (size 1.27 1.27))))
        (number "132" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -17.78 180) (length 5.08)
        (name "PT13B" (effects (font (size 1.27 1.27))))
        (number "133" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -20.32 180) (length 5.08)
        (name "PT13A" (effects (font (size 1.27 1.27))))
        (number "134" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -50.8 180) (length 5.08)
        (name "GNDIO02" (effects (font (size 1.27 1.27))))
        (number "135" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -45.72 180) (length 5.08)
        (name "VCCIO02" (effects (font (size 1.27 1.27))))
        (number "136" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -22.86 180) (length 5.08)
        (name "PT9B" (effects (font (size 1.27 1.27))))
        (number "137" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -25.4 180) (length 5.08)
        (name "PT9A" (effects (font (size 1.27 1.27))))
        (number "138" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -27.94 180) (length 5.08)
        (name "PT7B" (effects (font (size 1.27 1.27))))
        (number "141" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -30.48 180) (length 5.08)
        (name "PT8B" (effects (font (size 1.27 1.27))))
        (number "142" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -33.02 180) (length 5.08)
        (name "PT7A" (effects (font (size 1.27 1.27))))
        (number "143" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -35.56 180) (length 5.08)
        (name "PT8A" (effects (font (size 1.27 1.27))))
        (number "144" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LFXP2-5E-6TN144C_3_0"
      (text "BANK2" (at 6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
      (text "BANK3" (at -6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
    )
    (symbol "LFXP2-5E-6TN144C_3_1"
      (rectangle (start 11.43 19.05) (end -11.43 -48.26)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at 16.51 -15.24 180) (length 5.08)
        (name "PR6B" (effects (font (size 1.27 1.27))))
        (number "100" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -17.78 180) (length 5.08)
        (name "PR7A" (effects (font (size 1.27 1.27))))
        (number "101" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -20.32 180) (length 5.08)
        (name "PR6A" (effects (font (size 1.27 1.27))))
        (number "102" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -22.86 180) (length 5.08)
        (name "PR5B" (effects (font (size 1.27 1.27))))
        (number "103" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -25.4 180) (length 5.08)
        (name "PR5A" (effects (font (size 1.27 1.27))))
        (number "104" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -40.64 180) (length 5.08)
        (name "VCCIO22" (effects (font (size 1.27 1.27))))
        (number "105" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -45.72 180) (length 5.08)
        (name "GNDIO22" (effects (font (size 1.27 1.27))))
        (number "106" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -27.94 180) (length 5.08)
        (name "PR2B" (effects (font (size 1.27 1.27))))
        (number "107" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -30.48 180) (length 5.08)
        (name "PR2A" (effects (font (size 1.27 1.27))))
        (number "108" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 12.7 0) (length 5.08)
        (name "PR24A" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 10.16 0) (length 5.08)
        (name "PR24B" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -45.72 0) (length 5.08)
        (name "GNDIO3" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -43.18 0) (length 5.08)
        (name "VCCIO3" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 7.62 0) (length 5.08)
        (name "PR14B" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 5.08 0) (length 5.08)
        (name "PR14A" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 12.7 180) (length 5.08)
        (name "PR12B" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 10.16 180) (length 5.08)
        (name "PR12A" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 7.62 180) (length 5.08)
        (name "PR11B" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 5.08 180) (length 5.08)
        (name "PR11A" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 2.54 180) (length 5.08)
        (name "PR10B" (effects (font (size 1.27 1.27))))
        (number "91" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 0 180) (length 5.08)
        (name "PR9B" (effects (font (size 1.27 1.27))))
        (number "92" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -2.54 180) (length 5.08)
        (name "PR10A" (effects (font (size 1.27 1.27))))
        (number "93" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -5.08 180) (length 5.08)
        (name "PR9A" (effects (font (size 1.27 1.27))))
        (number "94" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -38.1 180) (length 5.08)
        (name "VCCIO21" (effects (font (size 1.27 1.27))))
        (number "95" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -7.62 180) (length 5.08)
        (name "PR8B" (effects (font (size 1.27 1.27))))
        (number "96" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -43.18 180) (length 5.08)
        (name "GNDIO21" (effects (font (size 1.27 1.27))))
        (number "97" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -10.16 180) (length 5.08)
        (name "PR8A" (effects (font (size 1.27 1.27))))
        (number "98" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -12.7 180) (length 5.08)
        (name "PR7B" (effects (font (size 1.27 1.27))))
        (number "99" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LFXP2-5E-6TN144C_4_0"
      (text "BANK4" (at 6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
      (text "BANK5" (at -6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
    )
    (symbol "LFXP2-5E-6TN144C_4_1"
      (rectangle (start 11.43 19.05) (end -11.43 -48.26)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -16.51 12.7 0) (length 5.08)
        (name "PB8A" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 10.16 0) (length 5.08)
        (name "PB7A" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 7.62 0) (length 5.08)
        (name "PB8B" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 5.08 0) (length 5.08)
        (name "PB7B" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -43.18 0) (length 5.08)
        (name "GNDIO51" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -38.1 0) (length 5.08)
        (name "VCCIO51" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 2.54 0) (length 5.08)
        (name "PB13B" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 0 0) (length 5.08)
        (name "PB13A" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -2.54 0) (length 5.08)
        (name "PB15A" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -5.08 0) (length 5.08)
        (name "PB14A" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -7.62 0) (length 5.08)
        (name "PB15B" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -10.16 0) (length 5.08)
        (name "PB14B" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -40.64 0) (length 5.08)
        (name "VCCIO52" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -12.7 0) (length 5.08)
        (name "PB16A" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -45.72 0) (length 5.08)
        (name "GNDIO52" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -15.24 0) (length 5.08)
        (name "PB16B" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -17.78 0) (length 5.08)
        (name "PB17A" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -20.32 0) (length 5.08)
        (name "PB17B" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -22.86 0) (length 5.08)
        (name "PB18A" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -25.4 0) (length 5.08)
        (name "PB19A" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -27.94 0) (length 5.08)
        (name "PB18B" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -30.48 0) (length 5.08)
        (name "PB19B" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 12.7 180) (length 5.08)
        (name "PB20A" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 10.16 180) (length 5.08)
        (name "PB20B" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -43.18 180) (length 5.08)
        (name "VCCIO4" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -45.72 180) (length 5.08)
        (name "GNDIO4" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 7.62 180) (length 5.08)
        (name "PB26A" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 5.08 180) (length 5.08)
        (name "PB26B" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 2.54 180) (length 5.08)
        (name "PB27A" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 0 180) (length 5.08)
        (name "PB28A" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -2.54 180) (length 5.08)
        (name "PB27B" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -5.08 180) (length 5.08)
        (name "PB28B" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LFXP2-5E-6TN144C_5_0"
      (text "BANK6" (at 6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
      (text "BANK7" (at -6.35 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
    )
    (symbol "LFXP2-5E-6TN144C_5_1"
      (rectangle (start 11.43 19.05) (end -11.43 -48.26)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -16.51 12.7 0) (length 5.08)
        (name "PL2A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -5.08 0) (length 5.08)
        (name "PL7B" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -7.62 0) (length 5.08)
        (name "PL8A" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -43.18 0) (length 5.08)
        (name "GNDIO71" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -10.16 0) (length 5.08)
        (name "PL8B" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -38.1 0) (length 5.08)
        (name "VCCIO71" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -12.7 0) (length 5.08)
        (name "PL9A" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -15.24 0) (length 5.08)
        (name "PL10A" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -17.78 0) (length 5.08)
        (name "PL9B" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -20.32 0) (length 5.08)
        (name "PL10B" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -22.86 0) (length 5.08)
        (name "PL11A" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 10.16 0) (length 5.08)
        (name "PL2B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -25.4 0) (length 5.08)
        (name "PL11B" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -27.94 0) (length 5.08)
        (name "PL12A" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -30.48 0) (length 5.08)
        (name "PL12B" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 12.7 180) (length 5.08)
        (name "PL15A" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 10.16 180) (length 5.08)
        (name "PL14A" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 7.62 180) (length 5.08)
        (name "PL15B" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -45.72 0) (length 5.08)
        (name "GNDIO72" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 5.08 180) (length 5.08)
        (name "PL14B" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 2.54 180) (length 5.08)
        (name "PL16B" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 0 180) (length 5.08)
        (name "PL16A" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -43.18 180) (length 5.08)
        (name "VCCIO6" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -45.72 180) (length 5.08)
        (name "GNDIO6" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -2.54 180) (length 5.08)
        (name "PL25A" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -5.08 180) (length 5.08)
        (name "PL25B" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 -40.64 0) (length 5.08)
        (name "VCCIO72" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 7.62 0) (length 5.08)
        (name "PL5A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 5.08 0) (length 5.08)
        (name "PL5B" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 2.54 0) (length 5.08)
        (name "PL6A" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 0 0) (length 5.08)
        (name "PL6B" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -2.54 0) (length 5.08)
        (name "PL7A" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LFXP2-5E-6TN144C_6_0"
      (text "JTAG" (at -7.62 16.51 0)
        (effects (font (size 1.524 1.524) italic))
      )
    )
    (symbol "LFXP2-5E-6TN144C_6_1"
      (rectangle (start 11.43 19.05) (end -11.43 -2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -16.51 2.54 0) (length 5.08)
        (name "TMS" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 5.08 0) (length 5.08)
        (name "TDI" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -16.51 0 0) (length 5.08)
        (name "TCK" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 7.62 0) (length 5.08)
        (name "TDO" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 12.7 0) (length 5.08)
        (name "VCCJ" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Lattice-JTAG" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "P" (id 0) (at -5.08 -8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "Lattice-JTAG" (id 1) (at 0 8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "Lattice-JTAG_0_1"
      (rectangle (start -6.35 7.62) (end 6.35 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Lattice-JTAG_1_1"
      (pin output clock (at -11.43 5.08 0) (length 5.08)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -5.08 180) (length 5.08)
        (name "PROG" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 5.08 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 2.54 0) (length 5.08)
        (name "TMS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 2.54 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 0 0) (length 5.08)
        (name "TDI" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 0 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 -2.54 0) (length 5.08)
        (name "TDO" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -2.54 180) (length 5.08)
        (name "INIT" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 -5.08 0) (length 5.08)
        (name "TRST" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
