(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MCP73833" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "MCP73833" (id 1) (at -1.27 -13.97 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -7.62 -1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22005b.pdf" (id 3) (at -7.62 -1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "ki_keywords" "Stand-Alone Linear Li-Ion / Li-Polymer Charge Management Controller" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "MCP73833" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP-10 DFN-10" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP73833_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -12.7)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP73833_1_1"
      (pin power_in line (at -12.7 5.08 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 2.54 180) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 2.54 0) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -12.7 -1.27 0) (length 5.08)
        (name "STAT1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -12.7 -3.81 0) (length 5.08)
        (name "STAT2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -10.16 0) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -10.16 180) (length 5.08)
        (name "PROG" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -12.7 -6.35 0) (length 5.08)
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -1.27 180) (length 5.08)
        (name "THERM" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 5.08 180) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
