(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "S25FL064LABNxxx-WSON_5x6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -11.43 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "S25FL064LABNxxx-WSON_5x6" (id 1) (at 1.27 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm" (id 2) (at 3.81 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/100/S25FL064L_64-Mbit_8-Mbyte_3.0_V_FL-L_SPI_Flash_Mem-1102570.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "64 Mbit SPI NOR Flash" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "S25FL064LABNxxx-WSON_5x6_0_1"
      (rectangle (start -11.43 8.89) (end 12.7 -10.16)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "S25FL064LABNxxx-WSON_5x6_1_1"
      (pin input line (at -16.51 6.35 0) (length 5.08)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 3.81 0) (length 5.08)
        (name "SO/IO1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -5.08 0) (length 5.08)
        (name "~{WP}/IO2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -7.62 180) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 1.27 0) (length 5.08)
        (name "SI" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -16.51 -1.27 0) (length 5.08)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -7.62 0) (length 5.08)
        (name "IO3/~{RESET}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 6.35 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -5.08 180) (length 5.08)
        (name "GNDPAD" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
