(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ADV7513" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ADV7513" (id 1) (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "LQFP-64_10x10mm_Pitch0.5mm_PAD" (id 2) (at -3.81 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.analog.com/en/products/audio-video/analoghdmidvi-interfaces/analog-hdmidvi-display-interfaces/adv7513.html" (id 3) (at 43.18 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Author" "Makise Kurisu <kurisu@shimatta.de>" (id 4) (at -1.27 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Version" "1.0" (id 5) (at -17.78 13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "HDMI PHY Transmitter Video TX" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ADV7513 HDMI Transmitter" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LQFP-64_10x10mm_Pitch0.5mm_PAD LQFP-64" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ADV7513_1_1"
      (rectangle (start -8.89 0) (end 8.89 -19.05)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -13.97 -2.54 0) (length 5.08)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -5.08 0) (length 5.08)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -10.16 180) (length 5.08)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -12.7 180) (length 5.08)
        (name "BGVDD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -2.54 180) (length 5.08)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -5.08 180) (length 5.08)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -7.62 180) (length 5.08)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -12.7 0) (length 5.08)
        (name "DVDD_3V" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -7.62 0) (length 5.08)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -10.16 0) (length 5.08)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -16.51 0) (length 5.08)
        (name "PAD/GND" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ADV7513_2_0"
      (rectangle (start -20.32 -116.84) (end 0 -101.6)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start -20.32 -24.13) (end 0 -101.6)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start -20.32 -24.13) (end 0 0)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start -20.32 0) (end 20.32 -116.84)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start -11.43 -114.935) (mid -10.9758 -114.7542) (end -10.795 -114.3)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -11.43 -5.715) (mid -10.9758 -5.5342) (end -10.795 -5.08)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -111.76) (mid -10.9758 -111.3058) (end -11.43 -111.125)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -2.54) (mid -10.9758 -2.0858) (end -11.43 -1.905)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -113.03) (mid -10.4177 -113.4073) (end -10.795 -114.3)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -30.48) (mid -10.4177 -30.8573) (end -10.795 -31.75)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -15.24) (mid -10.4177 -15.6173) (end -10.795 -16.51)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -3.81) (mid -10.4177 -4.1873) (end -10.795 -5.08)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -12.065 -107.95)
          (xy -9.525 -107.95)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -114.935)
          (xy -12.065 -114.935)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -111.125)
          (xy -12.065 -111.125)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -5.715)
          (xy -12.065 -5.715)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -1.905)
          (xy -12.065 -1.905)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -31.75)
          (xy -10.795 -33.655)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -27.305)
          (xy -10.795 -29.21)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -16.51)
          (xy -10.795 -20.955)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -9.525)
          (xy -10.795 -13.97)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -9.525 -104.14)
          (xy -12.065 -104.14)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 9.525 -50.165)
          (xy 9.525 -59.055)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 9.525 -38.735)
          (xy 9.525 -47.625)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -80.645)
          (xy 10.795 -80.645)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -76.835)
          (xy 10.795 -76.835)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -66.675)
          (xy 10.795 -66.675)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -62.865)
          (xy 10.795 -62.865)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.795 -73.66)
          (xy 8.255 -73.66)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.795 -69.85)
          (xy 8.255 -69.85)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -80.01) (mid 9.1659 -79.0991) (end 8.255 -78.74)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -80.01) (mid 9.7234 -80.4466) (end 10.16 -80.645)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -66.04) (mid 9.1659 -65.1291) (end 8.255 -64.77)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -66.04) (mid 9.7234 -66.4766) (end 10.16 -66.675)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 10.16 -76.835) (mid 9.7234 -77.0334) (end 9.525 -77.47)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 10.16 -62.865) (mid 9.7234 -63.0634) (end 9.525 -63.5)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 20.32 -35.56) (end 0 -82.55)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "Audio input" (at -2.54 -12.7 900)
        (effects (font (size 2.0066 2.0066) italic))
      )
      (text "Blue" (at -6.985 -46.99 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Calib." (at 4.445 -73.66 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "CEC" (at 5.715 -78.74 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Control" (at -5.715 -30.48 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Control" (at -2.54 -109.22 900)
        (effects (font (size 2.0066 2.0066) italic))
      )
      (text "DDC" (at 5.715 -64.77 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Green" (at -6.35 -68.58 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "HDMI" (at 2.54 -55.88 900)
        (effects (font (size 2.0066 2.0066) italic))
      )
      (text "Hotplg" (at 4.445 -69.85 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "I2C" (at -7.62 -113.03 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "I2S" (at -7.62 -15.24 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "IRQ" (at -7.62 -107.95 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Pwr" (at -7.62 -104.14 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Red" (at -6.985 -90.17 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "SPDIF" (at -6.35 -3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "TMDS" (at 5.08 -48.895 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Video input" (at -2.54 -55.88 900)
        (effects (font (size 2.0066 2.0066) italic))
      )
    )
    (symbol "ADV7513_2_1"
      (arc (start -12.065 -99.695) (mid -11.1723 -99.3177) (end -10.795 -98.425)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -12.065 -78.105) (mid -11.1723 -77.7277) (end -10.795 -76.835)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -12.065 -56.515) (mid -11.1723 -56.1377) (end -10.795 -55.245)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -12.065 -34.925) (mid -11.1723 -34.5477) (end -10.795 -33.655)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -12.065 -22.225) (mid -11.1723 -21.8477) (end -10.795 -20.955)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -111.76) (mid -10.4177 -112.6527) (end -9.525 -113.03)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -88.9) (mid -10.4177 -89.7927) (end -9.525 -90.17)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -81.915) (mid -11.1541 -81.0041) (end -12.065 -80.645)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -67.31) (mid -10.4177 -68.2027) (end -9.525 -68.58)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -60.325) (mid -11.1541 -59.4141) (end -12.065 -59.055)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -45.72) (mid -10.4177 -46.6127) (end -9.525 -46.99)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -38.735) (mid -11.1541 -37.8241) (end -12.065 -37.465)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -29.21) (mid -10.4177 -30.1027) (end -9.525 -30.48)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -27.305) (mid -11.1541 -26.3941) (end -12.065 -26.035)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -13.97) (mid -10.4177 -14.8627) (end -9.525 -15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -9.525) (mid -11.1541 -8.6141) (end -12.065 -8.255)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -10.795 -2.54) (mid -10.4177 -3.4327) (end -9.525 -3.81)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -90.17) (mid -10.4177 -90.5473) (end -10.795 -91.44)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -68.58) (mid -10.4177 -68.9573) (end -10.795 -69.85)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -9.525 -46.99) (mid -10.4177 -47.3673) (end -10.795 -48.26)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -98.425)
          (xy -10.795 -91.44)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -88.9)
          (xy -10.795 -81.915)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -76.835)
          (xy -10.795 -69.85)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -67.31)
          (xy -10.795 -60.325)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -55.245)
          (xy -10.795 -48.26)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.795 -45.72)
          (xy -10.795 -38.735)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 8.255 -78.74) (mid 9.1659 -78.3809) (end 9.525 -77.47)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 8.255 -64.77) (mid 9.1659 -64.4109) (end 9.525 -63.5)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 8.255 -48.895) (mid 9.1659 -48.5359) (end 9.525 -47.625)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -59.055) (mid 9.8841 -59.9659) (end 10.795 -60.325)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 9.525 -50.165) (mid 9.1659 -49.2541) (end 8.255 -48.895)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 10.795 -37.465) (mid 9.9023 -37.8423) (end 9.525 -38.735)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin input line (at -25.4 -21.59 0) (length 5.08)
        (name "LRCLK" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 25.4 -73.66 180) (length 5.08)
        (name "R_EXT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 25.4 -69.85 180) (length 5.08)
        (name "HPD" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -38.1 180) (length 5.08)
        (name "TXC-" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -40.64 180) (length 5.08)
        (name "TXC+" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -29.21 0) (length 5.08)
        (name "VSYNC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -44.45 180) (length 5.08)
        (name "TX0-" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -46.99 180) (length 5.08)
        (name "TX0+" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -104.14 0) (length 5.08)
        (name "PD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -50.8 180) (length 5.08)
        (name "TX1-" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -53.34 180) (length 5.08)
        (name "TX1+" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -57.15 180) (length 5.08)
        (name "TX2-" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -59.69 180) (length 5.08)
        (name "TX2+" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -25.4 -107.95 0) (length 5.08)
        (name "INT" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -2.54 0) (length 5.08)
        (name "SPDIF" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -77.47 180) (length 5.08)
        (name "CEC" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 25.4 -80.01 180) (length 5.08)
        (name "CEC_CLK" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 25.4 -63.5 180) (length 5.08)
        (name "DDCSCL" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -66.04 180) (length 5.08)
        (name "DDCSDA" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -25.4 -111.76 0) (length 5.08)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -114.3 0) (length 5.08)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -38.1 0) (length 5.08)
        (name "DATA0" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -40.64 0) (length 5.08)
        (name "DATA1" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -43.18 0) (length 5.08)
        (name "DATA2" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -5.08 0) (length 5.08)
        (name "MCLK" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -45.72 0) (length 5.08)
        (name "DATA3" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -48.26 0) (length 5.08)
        (name "DATA4" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -50.8 0) (length 5.08)
        (name "DATA5" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -53.34 0) (length 5.08)
        (name "DATA6" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -55.88 0) (length 5.08)
        (name "DATA7" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -59.69 0) (length 5.08)
        (name "DATA8" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -62.23 0) (length 5.08)
        (name "DATA9" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -64.77 0) (length 5.08)
        (name "DATA10" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -67.31 0) (length 5.08)
        (name "DATA11" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -69.85 0) (length 5.08)
        (name "DATA12" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -8.89 0) (length 5.08)
        (name "I2S0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -72.39 0) (length 5.08)
        (name "DATA13" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -74.93 0) (length 5.08)
        (name "DATA14" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -25.4 -26.67 0) (length 5.08)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -77.47 0) (length 5.08)
        (name "DATA15" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -81.28 0) (length 5.08)
        (name "DATA16" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -83.82 0) (length 5.08)
        (name "DATA17" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -86.36 0) (length 5.08)
        (name "DATA18" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -88.9 0) (length 5.08)
        (name "DATA19" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -91.44 0) (length 5.08)
        (name "DATA20" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -11.43 0) (length 5.08)
        (name "I2S1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -93.98 0) (length 5.08)
        (name "DATA21" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -96.52 0) (length 5.08)
        (name "DATA22" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -99.06 0) (length 5.08)
        (name "DATA23" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -34.29 0) (length 5.08)
        (name "DE" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -31.75 0) (length 5.08)
        (name "HSYNC" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -13.97 0) (length 5.08)
        (name "I2S2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -16.51 0) (length 5.08)
        (name "I2S3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -19.05 0) (length 5.08)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "IP4283CZ10" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IP4283CZ10" (id 1) (at 15.24 0 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at -13.97 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at -13.97 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IP4283CZ10_0_1"
      (rectangle (start -13.97 5.08) (end 13.97 -6.35)
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -11.43 2.54)
          (xy -8.89 2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -3.81)
          (xy -10.16 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 2.54)
          (xy -10.16 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 2.54)
          (xy -8.89 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 3.81)
          (xy -10.16 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 3.81)
          (xy 10.16 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 -2.54)
          (xy -10.16 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -6.35 2.54)
          (xy -3.81 2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -3.81)
          (xy -5.08 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54)
          (xy -5.08 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54)
          (xy -3.81 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 3.81)
          (xy -5.08 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 -2.54)
          (xy -5.08 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 1.27)
          (xy 0 -3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 1.27 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 2.54)
          (xy 1.27 1.905)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 6.35 2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -3.81)
          (xy 5.08 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 5.08 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 6.35 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 6.35 -2.54)
          (xy 5.08 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.89 2.54)
          (xy 11.43 2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -3.81)
          (xy -10.16 -3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -3.81)
          (xy 10.16 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 2.54)
          (xy 10.16 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 2.54)
          (xy 11.43 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 3.81)
          (xy 10.16 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -2.54)
          (xy 10.16 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 3.81)
          (xy 11.43 3.81)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -1.27)
          (xy -11.43 -2.54)
          (xy -8.89 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -1.27)
          (xy -11.43 -1.27)
          (xy -8.89 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 0)
          (xy -12.7 0)
          (xy -12.7 5.08)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 1.27)
          (xy -10.16 0)
          (xy -10.16 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 2.54)
          (xy -11.43 1.27)
          (xy -8.89 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -1.27)
          (xy -6.35 -2.54)
          (xy -3.81 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -1.27)
          (xy -6.35 -1.27)
          (xy -3.81 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 0)
          (xy -7.62 0)
          (xy -7.62 5.08)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 1.27)
          (xy -5.08 0)
          (xy -5.08 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54)
          (xy -6.35 1.27)
          (xy -3.81 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -3.81)
          (xy -1.27 -5.08)
          (xy -1.27 -6.35)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -3.81)
          (xy 1.27 -5.08)
          (xy 1.27 -6.35)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy -1.27 1.27)
          (xy 1.27 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy -1.27 2.54)
          (xy 1.27 2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -1.27)
          (xy 3.81 -2.54)
          (xy 6.35 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -1.27)
          (xy 3.81 -1.27)
          (xy 6.35 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 7.62 0)
          (xy 7.62 5.08)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 1.27)
          (xy 5.08 0)
          (xy 5.08 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 1.27)
          (xy 6.35 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -1.27)
          (xy 8.89 -2.54)
          (xy 11.43 -2.54)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -1.27)
          (xy 8.89 -1.27)
          (xy 11.43 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 0)
          (xy 12.7 0)
          (xy 12.7 5.08)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 1.27)
          (xy 10.16 0)
          (xy 10.16 -1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 2.54)
          (xy 8.89 1.27)
          (xy 11.43 1.27)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "IP4283CZ10_1_1"
      (pin input line (at -12.7 7.62 270) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 7.62 270) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -1.27 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 7.62 270) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 270) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 1.27 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -8.89 90) (length 2.54)
        (name "" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TMDS261B" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 38.1 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TMDS261B" (id 1) (at 30.48 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TMDS261B_0_0"
      (polyline
        (pts
          (xy 34.29 -35.56)
          (xy 34.29 -48.26)
          (xy 35.56 -48.26)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 26.67 -35.56)
          (xy 34.29 -35.56)
          (xy 34.29 -24.13)
          (xy 35.56 -24.13)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "1" (at 24.13 -29.21 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "2" (at 24.13 -43.18 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "TMDS261B_0_1"
      (polyline
        (pts
          (xy 8.89 -43.18)
          (xy 22.86 -43.18)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 26.67 -25.4)
          (xy 26.67 -48.26)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 -30.48)
          (xy 8.89 -30.48)
          (xy 8.89 -54.61)
          (xy 7.62 -54.61)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 -2.54)
          (xy 8.89 -2.54)
          (xy 8.89 -26.67)
          (xy 7.62 -26.67)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 8.89 -13.97)
          (xy 15.24 -13.97)
          (xy 15.24 -29.21)
          (xy 22.86 -29.21)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 26.67 -25.4)
          (xy 22.86 -22.86)
          (xy 22.86 -50.8)
          (xy 26.67 -48.26)
        )
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 0 0) (end 43.18 -100.33)
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TMDS261B_1_1"
      (pin no_connect line (at 48.26 -76.2 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -60.96 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -58.42 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -82.55 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -55.88 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -53.34 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -87.63 0) (length 5.08)
        (name "VSadj" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.26 -44.45 180) (length 5.08)
        (name "D2_S+" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 48.26 -46.99 180) (length 5.08)
        (name "D2_S-" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -85.09 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -73.66 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.26 -38.1 180) (length 5.08)
        (name "D1_S+" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 48.26 -40.64 180) (length 5.08)
        (name "D1_S-" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.59 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.26 -31.75 180) (length 5.08)
        (name "D0_S+" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 48.26 -34.29 180) (length 5.08)
        (name "D0_S-" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -87.63 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.26 -25.4 180) (length 5.08)
        (name "CLK_S+" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 48.26 -27.94 180) (length 5.08)
        (name "CLK_S-" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 24.13 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at 48.26 -2.54 180) (length 5.08)
        (name "SCL_S" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 48.26 -5.08 180) (length 5.08)
        (name "SDA_S" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 48.26 -19.05 180) (length 5.08)
        (name "HPD_SINK" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -82.55 0) (length 5.08)
        (name "S1/SCL" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -85.09 0) (length 5.08)
        (name "S2/SDA" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -80.01 0) (length 5.08)
        (name "I2C_SEL" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.08 -58.42 0) (length 5.08)
        (name "HPD1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -67.31 0) (length 5.08)
        (name "SDA1" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -5.08 -64.77 0) (length 5.08)
        (name "SCL1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted_clock (at -5.08 -6.35 0) (length 5.08)
        (name "CLK1-" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -5.08 -3.81 0) (length 5.08)
        (name "CLK1+" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -71.12 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -90.17 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -12.7 0) (length 5.08)
        (name "D0_1-" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -10.16 0) (length 5.08)
        (name "D0_1+" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 26.67 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -19.05 0) (length 5.08)
        (name "D1_1-" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -16.51 0) (length 5.08)
        (name "D1_1+" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -92.71 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -25.4 0) (length 5.08)
        (name "D2_1-" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -22.86 0) (length 5.08)
        (name "D2_1+" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at 48.26 -12.7 180) (length 5.08)
        (name "~{LP}" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -68.58 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.08 -60.96 0) (length 5.08)
        (name "HPD2" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -73.66 0) (length 5.08)
        (name "SDA2" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -5.08 -71.12 0) (length 5.08)
        (name "SCL2" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted_clock (at -5.08 -34.29 0) (length 5.08)
        (name "CLK2-" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -5.08 -31.75 0) (length 5.08)
        (name "CLK2+" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -95.25 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -40.64 0) (length 5.08)
        (name "D0_2-" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -38.1 0) (length 5.08)
        (name "D0_2+" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 29.21 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -46.99 0) (length 5.08)
        (name "D1_2-" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -80.01 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -44.45 0) (length 5.08)
        (name "D1_2+" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 48.26 -97.79 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.08 -53.34 0) (length 5.08)
        (name "D2_2-" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -50.8 0) (length 5.08)
        (name "D2_2+" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -50.8 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -66.04 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 48.26 -63.5 180) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 -105.41 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
