(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "AP63300" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 10.16 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AP63300" (id 1) (at 3.81 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AP63300_0_1"
      (rectangle (start 0 0) (end 15.24 -16.51)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "AP63300_1_1"
      (pin input line (at 20.32 -13.97 180) (length 5.08)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -5.08 0) (length 5.08)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -13.97 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 20.32 -8.89 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -2.54 180) (length 5.08)
        (name "BST" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LDK220-SOT89" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LDK220-SOT89" (id 1) (at 8.89 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LDK220-SOT89_0_1"
      (rectangle (start 0 0) (end 10.16 -8.89)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LDK220-SOT89_1_1"
      (pin power_out line (at 12.7 -2.54 180) (length 2.54)
        (name "Vout" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -11.43 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -2.54 0) (length 2.54)
        (name "Vin" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LM2596" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LM2596" (id 1) (at 3.81 8.89 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -1.27 5.08 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf" (id 3) (at -1.27 5.08 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "ki_keywords" "Buck Step-down regulator" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LM2596 SIMPLE SWITCHER ® Power Converter 150 kHz 3A Step-Down Voltage Regulator" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DDPAK TO-263" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM2596_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LM2596_1_1"
      (pin power_in line (at -12.7 2.54 0) (length 5.08)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 0 180) (length 5.08)
        (name "Output" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -12.7 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 5.08 180) (length 5.08)
        (name "Feedback" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -3.81 -12.7 90) (length 5.08)
        (name "ON" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LP2985" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LP2985" (id 1) (at 11.43 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 11.43 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp2985.pdf?HQS=TI-null-null-mousermode-df-pf-null-wwe&ts=1607253562710&ref_url=https%253A%252F%252Fno.mouser.com%252F" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ldo,low noise,regulator" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LP2985 150-mA Low-noise Low-dropout Regulator With Shutdown" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LP2985_0_1"
      (rectangle (start 0 0) (end 22.86 -13.97)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LP2985_1_1"
      (pin power_in line (at -2.54 -2.54 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -11.43 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -5.08 0) (length 2.54)
        (name "ON/~{OFF}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 25.4 -11.43 180) (length 2.54)
        (name "BYPASS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 25.4 -2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LP8867" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LP8867" (id 1) (at 6.35 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LP8867_0_1"
      (rectangle (start 0 0) (end 19.05 -33.02)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "LP8867_1_1"
      (pin power_in line (at -2.54 -2.54 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -21.59 0) (length 2.54)
        (name "ISET" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -35.56 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 21.59 -19.05 180) (length 2.54)
        (name "OUT4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 21.59 -16.51 180) (length 2.54)
        (name "OUT3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 21.59 -13.97 180) (length 2.54)
        (name "OUT2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 21.59 -11.43 180) (length 2.54)
        (name "OUT1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -5.08 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.24 -35.56 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 21.59 -2.54 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -30.48 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -24.13 0) (length 2.54)
        (name "LDO" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -35.56 90) (length 2.54)
        (name "GNDPAD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -11.43 0) (length 2.54)
        (name "FSET" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -8.89 0) (length 2.54)
        (name "VDDIO/EN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector output_low (at -2.54 -13.97 0) (length 2.54)
        (name "FAULT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -16.51 0) (length 2.54)
        (name "SYNC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -19.05 0) (length 2.54)
        (name "PWM" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -27.94 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -35.56 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LTC3612-TSSOP" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 22.86 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LTC3612-TSSOP" (id 1) (at 10.16 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "http://cds.linear.com/docs/en/datasheet/3612fc.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_keywords" "regulator, dc-dc" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "The LTC3612 is a low quiescent current monolithic synchronous buck regulator using a current mode, constant frequency architecture." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC3612-TSSOP_0_1"
      (rectangle (start 0 0) (end 25.4 -30.48)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
    )
    (symbol "LTC3612-TSSOP_1_1"
      (pin power_in line (at -5.08 -1.27 0) (length 5.08)
        (name "SVin" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.24 -35.56 90) (length 5.08)
        (name "SGND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 30.48 -1.27 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 30.48 -3.81 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -8.89 0) (length 5.08)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -6.35 0) (length 5.08)
        (name "PVIN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 30.48 -6.35 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 30.48 -8.89 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -17.78 0) (length 5.08)
        (name "RUN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -3.81 0) (length 5.08)
        (name "PVIN_DRV" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -35.56 90) (length 5.08)
        (name "PGND-Pad" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -5.08 -12.7 0) (length 5.08)
        (name "PGOOD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -20.32 0) (length 5.08)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -22.86 0) (length 5.08)
        (name "VFB" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -25.4 0) (length 5.08)
        (name "ITH" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -15.24 0) (length 5.08)
        (name "TRACK/SS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 30.48 -26.67 180) (length 5.08)
        (name "DDR" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -27.94 0) (length 5.08)
        (name "RT/SYNC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MC34063" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 13.97 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "MC34063" (id 1) (at 5.08 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "MC34063_0_1"
      (rectangle (start 0 0) (end 26.67 -12.7)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "MC34063_1_1"
      (pin power_in line (at -5.08 -1.27 0) (length 5.08)
        (name "Switch_Coll" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 31.75 -3.81 180) (length 5.08)
        (name "Switch_Emitter" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -8.89 0) (length 5.08)
        (name "T_Cap" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 31.75 -11.43 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 31.75 -7.62 180) (length 5.08)
        (name "COMP_IN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -11.43 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -6.35 0) (length 5.08)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -3.81 0) (length 5.08)
        (name "Drive_Coll" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MCP1799-SOT23" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MCP1799-SOT23" (id 1) (at 6.35 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.de/datasheet/2/268/MCP1799_Data_Sheet_20006248B-2887414.pdf" (id 3) (at -0.635 5.715 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "80 mA High-Voltage Automotive LDO" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MCP1799-SOT23_0_1"
      (rectangle (start 0 0) (end 12.7 -8.89)
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "MCP1799-SOT23_1_1"
      (pin power_in line (at 6.35 -11.43 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 15.24 -2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -2.54 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MMTL431A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MMTL431A" (id 1) (at 7.62 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MMTL431A_0_1"
      (polyline
        (pts
          (xy -2.54 0)
          (xy 2.54 0)
          (xy 2.54 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 2.54)
          (xy 2.54 2.54)
          (xy 0 0)
          (xy -2.54 2.54)
          (xy -1.27 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "MMTL431A_1_1"
      (pin passive line (at -6.35 1.27 0) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 90) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 5.08 270) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SIM2-XXXXD" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 17.78 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "SIM2-XXXXD" (id 1) (at 7.62 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "SIM2-XXXXD_0_1"
      (rectangle (start 0 0) (end 17.78 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SIM2-XXXXD_1_1"
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "VIN+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "VIN-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -6.35 180) (length 5.08)
        (name "VOUT-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -3.81 180) (length 5.08)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -1.27 180) (length 5.08)
        (name "VOUT+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ST1S10" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "ST1S10" (id 1) (at 12.7 1.27 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/fb/03/25/5a/eb/45/46/33/CD00169322.pdf/files/CD00169322.pdf/jcr:content/translations/en.CD00169322.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_keywords" "Step Down Switch Mode Power Supply SMPS" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "3 A, 900 kHz, monolithic synchronous step-down regulator IC" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "PowerSO-8" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ST1S10_0_1"
      (rectangle (start 0 0) (end 15.24 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ST1S10_1_1"
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "V_IN_A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -10.16 0) (length 5.08)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -10.16 180) (length 5.08)
        (name "V_FB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -22.86 90) (length 5.08)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -22.86 90) (length 5.08)
        (name "SYNC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "V_IN_SW" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 20.32 -2.54 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 3.81 -22.86 90) (length 5.08)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TBA1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TBA1" (id 1) (at 2.54 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TBA1_0_1"
      (rectangle (start 0 0) (end 16.51 -6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TBA1_1_1"
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "VIN-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -1.27 0) (length 5.08)
        (name "VIN+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 21.59 -5.08 180) (length 5.08)
        (name "VOUT-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 21.59 -1.27 180) (length 5.08)
        (name "VOUT+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS54227" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 12.7 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS54227" (id 1) (at 5.08 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS54227_0_1"
      (rectangle (start 0 0) (end 16.51 -19.05)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS54227_1_1"
      (pin input line (at -2.54 -2.54 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -5.08 0) (length 2.54)
        (name "VFB" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -7.62 0) (length 2.54)
        (name "VREG5" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -11.43 0) (length 2.54)
        (name "SS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 -21.59 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 19.05 -7.62 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 -5.08 180) (length 2.54)
        (name "VBST" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 -2.54 180) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -21.59 90) (length 2.54)
        (name "Pad" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS562231" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS562231" (id 1) (at 10.16 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS562231_0_1"
      (rectangle (start 0 0) (end 17.78 -15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS562231_1_1"
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -7.62 180) (length 5.08)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -2.54 180) (length 5.08)
        (name "BST" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -7.62 0) (length 5.08)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -12.7 180) (length 5.08)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
